
SIFS v1.1 - SIEMENS Flex-Filesystem via OBEX
--------------------------------------------
Copyright (c)2003 Andreas Ziemer
eMail: sifs@a-z-e.de

This Total Commander plugin gives access to SIEMENS mobile phones
with flexmemory, ME45, S45 and others.
(ERICSSON T68 not tested - gimme feedback !)

Requires TotalCommander v5.51 or later!


Installation
============
1) Copy SIFS.WFX to a folder of your choice, best is Total Commander folder.
2) From Total Commander's main menu, select
    Configuration -> Operation -> FS-Plugins
3) In the popup box press 'Add', locate and select SIFS.WFX and press OK.

After the first start you have to select the COM-port where your mobile
is connected to, and the baud rate. SIEMENS currently supports 57600 and
19200, ERICSSON needs 19200 (untested). Later SIEMENS phones as the 45 series
might work with 115200 (also untested).

Hint: To change COM port or speed later, press and hold the right mouse
button on the FlexMem entry in Network Neighbourhood, then click Properties.

Legal disclaimer:
-----------------
This program is distributed in the hope that it will be useful,
but WITHOUT ANY WARRANTY; without even the implied warranty of
MERCHANTABILITY or FITNESS FOR ANY PARTICULAR PURPOSE.

This program contains the OpenOBEX library (GNU GPL) and parts of
OpenOBEX COBEX (GNU GPL). See attached files for more information.


Version history
---------------

1.1:	Fixed problem when copying/moving/renaming within FlexMem
1.0:	First official release version
	Significant speed improvement
	Progress bar
0.9b3:	Intermediate version
0.9b2:	Fixed a bug when creating directories
0.9b1:	Initial release
